{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":41,"n_cols":3,"rows_kept":41,"cut":false,"hidden":false,"merged":[[0,0,0,3],[1,0,1,3],[2,0,2,3],[40,0,40,3],[4,0,4,3],[23,0,25,3],[26,0,26,3],[36,0,39,3],[5,0,5,3]],"flags":["formulas_cached_only"]}
["United States"]
["ENVIRONMENTAL PROTECTION AGENCY"]
["Washington, D.C. 20460"]
[]
["ENERGY STAR Ventilating Fan Partner\nUnit Shipment Data"]
["Office of Atmospheric Programs"]
[]
["NAME OF MANUFACTURER:"]
[]
["DATE OF SUBMISSION:"]
[]
["SUBMITTED BY (NAME):"]
[]
["Reporting Period: CALENDAR YEAR 2007 (JAN. TO DEC.)"]
["Ventilating Fan1 Product Type","ENERGY STAR® U.S. Unit Shipments                     (REQUIRED)","Total U.S. Unit Shipments (ENERGY STAR + Non-ENERGY STAR)         (REQUESTED)"]
["Range Hoods - up to 500 cfm (max)"]
["Bathroom and Utility Room Fans - 10 to 80 cfm"]
["Bathroom and Utility Room Fans - 90 to 130 cfm"]
["Bathroom and Utility Room Fans - 140 to 500 cfm (max)"]
["In-Line Ventilating Fans - single-port2"]
["In-Line Ventilating Fans - multi-port3"]
["Total"]
["DEFINITIONS"]
["1 A ceiling, wall-mounted, or remotely mounted in-line fan designed to be used in a bathroom or utility room, or a kitchen range hood, whose purpose is to move objectionable air from inside the building to the outdoors.  Residential ventilating fans used for cooling (e.g., whole-house fans) or air circulation are excluded.  Heat/energy recovery ventilation fans ducted to the ventilated space, powered attic ventilators (e.g., gable fans), residential ventilating fans with heat lamps are excluded.  This definition does not address passive ventilation of any kind."]
[]
[]
["2, 3 A fan designed to be located within the building structure and requires ductwork on both intake and exhaust.  Those inline fans with only one intake are referred to as \"single port\" in-line fans, while those with multiple intake ports are referred to as \"multi-port\" in-line fans."]
["Submission Deadline: March 31, 2008"]
["Please submit by mail, email, or fax to:"]
["Elliott Rector"]
["ICF International"]
["1725 Eye Street, NW"]
["Suite 1000"]
["Washington, DC 20006"]
["unitshipmentdata@icfi.com"]
["Fax: (202) 862-1144"]
["Any information submitted to EPA for which a claim of confidentiality is made will be safeguarded according to the Agency policies set forth in Title 40, chapter 1, part 1, subpart B - Confidentiality of Business Information (see 40 CFR part 2; 41 FR 36902, September 1, 1976; amended by 43 FR 40000, September 8, 1978; 43 FR 42251, September 20, 1978; 44 FR 17674, March 23, 1979)."]
[]
[]
[]
["The public reporting and recordkeeping burden for this collection of information is estimated to average 6.7 hours per response. Send comments on the Agency's need for this information, the accuracy of the provided burden estimates, and any suggested methods for minimizing respondent burden, including through the use of automated collection techniques to the Director, Collection Strategies Division, U.S. Environmental Protection Agency (2822T), 1200 Pennsylvania Ave., NW, Washington, D.C. 20460. Include the OMB control number in any correspondence. Do not send the completed form to this address."]