{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[[1,2,1,3],[1,4,1,6]],"flags":["formulas_cached_only"]}
["ENERGY STAR ICR Increase"]
[null,null,"Hr and Cost /Respondent",null,"Total Hour and Costs"]
["Form","EPA Form #","Respond Hr/Yr","Labor Costs/Yr","Number of Respondents","Total Respondent Hours/Year","Total Cost/Year"]
["Imaging USD","5900-163",14.5,736.98,45,652.5,33164.1]
[]
["Comm Dishwasher USD","5900-164",14.5,736.98,15,217.5,11054.7]
[]
["Computers USD","5900-165",14.5,736.98,85,1232.5,62643.3]
[]
["Dec Lights USD","5900-166",14.5,736.98,15,217.5,11054.7]
[]
["DTA USD","5900-167",14.5,736.98,9,130.5,6632.82]
[]
["Comm Ice Machine USD","5900-168",14.5,736.98,6,87,4421.88]
[]
["Comm Dishwasher QPI","5900-169",11.25,746.06,237,2666.25,176816.22]
[]
["Comm Ice Machine QPI","5900-170",11.25,746.06,162,1822.5,120861.71999999999]
[]
["Battery Chargers QPI","5900-171",11.25,746.06,81,911.25,60430.85999999999]
[]
["Totals",null,120.75,null,655,7937.5,487080.29999999993]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}