{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["FGIS-927","Instructions","link3"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":1,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"FGIS-927","index":0,"n_rows":41,"n_cols":37,"rows_kept":41,"cut":false,"hidden":false,"merged":[[33,19,33,21],[34,11,34,18],[34,19,34,21],[33,0,33,7],[34,0,34,7],[33,8,33,10],[34,8,34,10],[22,22,23,37],[35,0,35,37],[33,25,34,37],[24,22,25,37],[32,5,32,7],[32,8,32,10],[32,13,32,15],[32,16,32,18],[32,19,32,21],[33,11,33,18],[40,0,40,37],[38,0,38,18],[31,35,31,37],[31,29,31,34],[32,35,32,37],[32,29,32,34],[32,0,32,1],[32,2,32,4],[36,24,36,37],[33,22,33,24],[29,22,29,25],[29,26,29,28],[29,29,29,31],[29,32,29,34],[30,22,30,34],[26,35,26,37],[27,22,27,25],[27,26,27,28],[27,29,27,31],[27,32,27,34],[26,22,26,25],[26,26,26,28],[26,29,26,31],[26,32,26,34],[27,35,27,37],[36,0,36,11],[37,0,37,11],[36,12,36,23],[37,12,37,23],[32,11,32,12],[31,11,31,12],[31,13,31,15],[31,16,31,18],[31,19,31,21],[30,11,30,12],[30,13,30,15],[30,16,30,18],[30,19,30,21],[29,11,29,12],[29,13,29,15],[29,16,29,18],[29,19,29,21],[28,11,28,12],[28,13,28,15],[28,16,28,18],[28,19,28,21],[27,11,27,12],[27,13,27,15],[27,16,27,18],[27,19,27,21],[23,11,23,21],[24,11,24,21],[25,11,25,21],[26,11,26,12],[26,13,26,15],[26,16,26,18],[26,19,26,21],[22,0,22,10],[23,0,23,10],[24,0,24,10],[25,0,25,10],[26,8,26,10],[27,8,27,10],[31,0,31,1],[31,2,31,4],[29,0,29,1],[29,2,29,4],[30,0,30,1],[30,2,30,4],[27,0,27,1],[27,2,27,4],[27,5,27,7],[28,0,28,1],[26,0,26,1],[26,2,26,4],[26,5,26,7],[28,22,28,25],[28,26,28,28],[28,29,28,31],[28,32,28,34],[28,35,28,37],[28,2,28,4],[37,24,37,33],[37,34,37,37],[28,5,28,7],[28,8,28,10],[29,5,29,7],[29,8,29,10],[29,35,29,37],[30,5,30,7],[30,8,30,10],[38,19,39,37],[39,0,39,3],[39,4,39,7],[39,9,39,12],[30,35,30,37],[31,5,31,7],[31,8,31,10],[31,22,31,28],[32,22,32,28],[17,30,18,31],[17,32,18,33],[17,34,18,35],[17,36,18,37],[13,30,14,33],[6,27,6,37],[5,27,5,37],[15,30,16,31],[15,32,16,33],[15,34,16,35],[15,36,16,37],[11,0,11,37],[12,0,12,37],[13,34,14,37],[9,0,9,37],[10,0,10,37],[5,0,5,8],[5,9,5,17],[5,18,5,26],[6,0,6,8],[6,9,6,17],[6,18,6,26],[7,0,8,37],[17,20,18,21],[17,22,18,23],[17,24,18,26],[17,27,18,29],[17,17,18,19],[13,20,13,23],[13,24,14,26],[13,27,14,29],[14,20,14,21],[14,22,14,23],[15,20,16,21],[15,22,16,23],[15,24,16,26],[15,27,16,29],[15,0,16,1],[15,2,16,3],[15,4,16,6],[13,7,14,9],[13,4,14,6],[13,0,13,3],[14,0,14,1],[14,2,14,3],[13,14,14,16],[13,17,14,19],[15,7,16,9],[15,10,16,11],[15,12,16,13],[15,14,16,16],[15,17,16,19],[14,10,14,11],[14,12,14,13],[13,10,13,13],[22,11,22,21],[17,0,18,1],[17,2,18,3],[17,4,18,6],[17,7,18,9],[19,0,19,37],[20,0,21,37],[17,10,18,11],[17,12,18,13],[17,14,18,16],[0,26,4,37],[0,0,0,25],[1,0,1,25],[2,0,2,25],[3,0,3,25],[4,0,4,25]],"flags":["formulas_cached_only"]}
["U.S. DEPARTMENT OF AGRICULTURE",{"$nulls":25},"FORM APPROVED OMB. 0580-0013\nAccording to the Paperwork Reduction Act of 1995, no persons are\nrequired to respond to a collection of information unless it displays a\nvalid OMB control number.  The valid OMB control number for this\ninformation is 0580-0013.  The time required to complete this\ninformation collection is estimated to average 5 minutes per response,\nincluding the time for reviewing instructions, search existing data\nsources, gathering and maintaining the data needed, and completing\nand reviewing the collection of information."]
["GRAIN INSPECTION, PACKERS AND STOCKYARDS ADMINISTRATION"]
["TESTWEIGHT CHECKTEST"]
[]
["NOTE:  TEST UNIT OPERATOR FILL IN SHADED AREAS ONLY"]
["DATE MAILED",{"$nulls":8},"FIELD OFFICE",{"$nulls":8},"AGENCY",{"$nulls":8},"LOCATION"]
[]
["SCALE / BEAM TEST\nBefore proceeding with test review Chapter 5 of the Equipment Handbook.  Clean, level and balance the scale, filling apparatus, and kettle.  Test weights must have a current Class F Report of Test."]
[]
["Scale Brand / Model / Serial No. /  Date of Test"]
[]
["Scale Test for Electronic or Mechanical Grain Scales:  This scale was tested in accordance with Chapter 2 of the Equipment Handbook and found to be within tolerance."]
["Beam Test:  Complete test below.  Tolerance is +/- 0.10 pound."]
["Load",null,null,null,"Beam\nReading",null,null,"Error",null,null,"Load",null,null,null,"Beam\nReading",null,null,"Error",null,null,"Load",null,null,null,"Beam\nReading",null,null,"Error",null,null,"Sensitivity\n@ 60 lb/bu",null,null,null,"Beam Response\nOK?"]
["g",null,"lb",{"$nulls":7},"g",null,"lb",{"$nulls":7},"g",null,"lb"]
[0,null,0,{"$nulls":4},"",null,null,142,null,10,{"$nulls":4},"",null,null,850,null,60,{"$nulls":4},"",null,null,"g",null,"lb",null,"Yes",null,"No"]
[]
[71,null,5,{"$nulls":4},"",null,null,425,null,30,{"$nulls":4},"",{"$nulls":9},"",null,null,"850+1 g",null,"60+1g"]
[]
["GRAIN TEST"]
["Before the Grain Test, check alignment of the funnel and kettle.  Record results to 0.00 pound for mechanical or electronic scales.  For beams, the 0.1 pound graduations should be estimated to ¼ graduations and\nrecorded as 0.025, 0.050, 0.075, or 0.100 pounds.  For each sample, strike the highest and lowest drops and average the remaining three results."]
[]
["TEST UNIT Beam  / Filler Brand & Serial No.",{"$nulls":10},"STANDARD UNIT Beam  / Filler Brand & Serial No.",{"$nulls":10},"TEST SUMMARY"]
[]
["Kettle Brand & Serial No.",{"$nulls":10},"Kettle Brand & Serial No."]
[]
["Drop",null,"Sample 1",null,null,"Sample 2",null,null,"Sample 3",null,null,"Drop",null,"Sample 1",null,null,"Sample 2",null,null,"Sample 3",{"$nulls":6},"Sample 1",null,null,"Sample 2",null,null,"Sample 3",null,null,"TOTAL"]
[1,{"$nulls":10},1,{"$nulls":10},"TEST UNIT",null,null,null,0,null,null,0,null,null,0,null,null,0]
[2,{"$nulls":10},2,{"$nulls":10},"STD. UNIT",null,null,null,0,null,null,0,null,null,0,null,null,0]
[3,{"$nulls":10},3,{"$nulls":10},"DIFFERENCE",null,null,null,0,null,null,0,null,null,0,null,null,0]
[4,{"$nulls":10},4,{"$nulls":10},"Mean Deviation from Standard (Total Diff.  3)"]
[5,{"$nulls":10},5,{"$nulls":10},"MDS Tolerance = 0.15 lb / bu",{"$nulls":6},"IN TOLERANCE"]
["Avg",{"$nulls":10},"Avg",{"$nulls":17},"OUT OF TOLERANCE"]
["Results By:",{"$nulls":7},"Date:",null,null,"Results By:",{"$nulls":7},"Date:",null,null,"Remarks"]
[]
["VOLUME TEST"]
["Scale Used in Test / Brand / Model / Serial No.",{"$nulls":11},"Kettle Brand & Serial No.",{"$nulls":11},"Results By:  /       Date of Test:"]
[]
["  GROSS              -  TARE              =                   NET WEIGHT (1,098.08 g at 68 °F)",{"$nulls":18},"OR                  Filled kettle ± 1.0 g of Standard counter weight."]
[{"$nulls":9},0,null,null,null,"g"]
["Form FGIS-927 (7-96)  Previous Editions are Obsolete."]

{"sheet":"Instructions","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"link3","index":2,"n_rows":1,"n_cols":9,"rows_kept":1,"cut":false,"hidden":true,"merged":[],"flags":["formulas_cached_only"]}
[0.4,{"$nulls":7},"№¼±°"]