{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":28,"n_cols":4,"rows_kept":28,"cut":false,"hidden":false,"merged":[[27,0,27,3],[1,1,1,3],[8,1,8,3],[14,1,14,3],[19,1,19,3]],"flags":["formulas_cached_only"]}
["New Requirement Description","Increased Cost Per Facility","Increased Costs For Industry","Cost Information"]
["Release Prevention"]
["Walk Through Inspections",3600,803365200,"Costs assume that a Third Party will need to perform the inspection. Typical station personel do not have the right work clasification to perform the inspection. It will cost $300 per month to hire contractor."]
["Over-Fill Prevention Equipment Tests",135,30126195,"The cost to have Overfill Prevention tested will be $400 to test three Overfill devices. Overfill only needs to be tested once every three years, therefore it will cost $135 annually."]
["Spill Prevention Equipment Tests",750,167367750,"It will cost $350 to have the Spill Buckets tested & $400 to dispose of waste. 20 gallons of waste water is antisipated to be generated by three Spill Buckets and one Stage I bucket. Disposal of one drum of waste water is $400."]
["Interstitial Integrity Tests",1050,234314850,"It will cost $250 per UST to test the interstitial space. It will also cost $100 per line to test the interstitial space and $2,100 to test 7 sumps and dispose of waste water. Based on three USTs, four dispensers it will cost $3,150 to test every three years or $1,050 annually."]
["Testing Repairs to Spill & Over-Fill Prevention Equipment and Interstices",175,null,"It will cost an additional $175 to have the repaired Spill Bucket or Overfill tested. We are assuming that the test will be performed by the technician doing the repair. If an independent contractor is required the cost would be $350."]
["Eliminate Flow Restrictors in Vent Lines for all New Tanks and When Over-fill Devices are Replaced",2200,null,"It will cost $650 per drop tube for materials and $250 in labor to install."]
["Release Detection"]
["Operability Tests for Release Detection Methods",300,66947100,"It cost $300 to have a contractor certify a typical Leak Detection system."]
["Add SIR/CITLD to Regulations with Performance Criteria"]
["Response to Interstitial Monitoring Alarms",350,null,"It will cost $350 to have a service contractor come to the site to investigate alarms. Many containment areas cannot be accesssed by station personel."]
["Eliminate groundwater and vapor monitoring as release detection methods "]
["Remove deferral for emergency generator tanks "]
["Other"]
["Require notification of ownership change ",100,null,"The cost represents the time it will take to fill out new Registration forms."]
["Closure of lined tanks that cannot be repaired according to a code of practice "]
["Requirements for determining compatibility "]
["Remove deferrals for airport hydrant fuel distribution systems and UST systems with field-constructed tanks "]
["EPA ct-related Provisions"]
["Operator training ",500,111578500,"It will cost $500 to provide training for Class A/B/C Operators that need to be certified."]
["Secondary containment "]
["Under Dispenser Containment for all New Dispensers"]
[]
["Annual Costs",6960,1553172720]
["One Time Costs",2200]
[]
["* The costs are based on Conventional UST Systems consisting of three USTs per system. Industry costs assumes 223,157 facilities."]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}