{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Phase 2 Credit Allowance"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Phase 2 Credit Allowance","index":0,"n_rows":48,"n_cols":9,"rows_kept":48,"cut":false,"hidden":false,"merged":[[36,3,40,8],[27,1,32,8],[35,3,35,8],[23,1,23,3],[10,2,10,3],[6,0,6,9],[24,1,24,2],[25,1,25,2],[1,0,1,9],[2,0,2,9],[3,0,3,9],[5,0,5,9]],"flags":["formulas_cached_only"]}
[]
["United States"]
["Environmental Protection Agency"]
["Office of Transportation and Air Quality"]
[]
["Manufacturer Averaging, Banking, and Trading Report for Small Spark Ignition Engines"]
["Last Revision: August 2010    Version Number: 2.3"]
[]
["Phase 2 Credit Allowance for Phase 3 Compliance",{"$nulls":6},"Submission Date:"]
[]
[null,"MANUFACTURER:"]
[]
[null,"Model Year","Engine Class","Emissions Delta (g/kW-hr)","Production Volume1","Avg Power (kW)2","Avg Useful Life (hrs)3","Load Factor","Credits"]
[null,2007,"I",1.6,{"$nulls":4},0]
[null,2008,"I",1.6,{"$nulls":4},0]
[null,2009,"I",1.6,{"$nulls":4},0]
[null,2007,"II",2.1,{"$nulls":4},0]
[null,2008,"II",2.1,{"$nulls":4},0]
[null,2009,"II",2.1,{"$nulls":4},0]
[null,"1 The Volume is the number of engines eligible to participate in the ABT program."]
[null,"2 The Avg Power should be the production-weighted average value of the maximum modal power for all engine families in the engine class."]
[null,"3 The Avg Useful Life should be the production-weighted average value of the useful life for all engine families in the engine class."]
[]
[null,"Total Allowable Phase 2 Credits"]
[null,"Class I Phase 2 Credits",null,0]
[null,"Class II Phase 2 Credits",null,0]
[]
[null,"This form should be completed only once at the end of the 2009 model year to determine the maximum number of Class I and Class II Phase 2 credits that may be used to demonstrate compliance with the Class I and Class II Phase 3 exhaust emission standards.  The number of credits calculated in this form does not represent the actual number of Class I and II Phase 2 credits a manufacturer owns; rather, it acts as a cap for the number of credits that may be applied for compliance.  The credits may be used in the 2012 and 2013 model years for Class I engines and in the 2011 through 2013 model years for Class II engines only after all transitional credits from engines meeting Phase 3 standards have been exhausted.  "]
{"$rows_empty":7}
[null,null,null,"Paperwork Reduction Act Notice"]
[null,null,null,"The public reporting and recordkeeping burden for this collection of information is estimated to average 26 hours per response.  Send comments on the Agency's need for this information, the accuracy of the provided burden estimates, and any suggested methods for minimizing respondent burden, including through the use of automated collection techniques to the Director, Collection Strategies Division, U.S. Environmental Protection Agency (2822T), 1200 Pennsylvania Ave., NW, Washington, D.C. 20460.  Include the OMB control number in any correspondence.  Do not send the completed Form to this address."]
[]
[]
[]
[]
[]
[]
[null,"Error Message: You have exceeded the number of Phase 2 Credits you are able to use."]
[null,"Error Message: You may use Phase 2 emission credits only in 2012 and 2013 for Class I engines."]
[null,"Error Message: You may use Phase 2 emission credits only in 2011 through 2013 for Class II engines."]
[]
[null,0.47]