{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Parts 1-5","Part 6","Part 7-8"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":3,"defined_names":14,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Parts 1-5","index":0,"n_rows":47,"n_cols":43,"rows_kept":47,"cut":false,"hidden":false,"merged":[[30,36,30,42],[17,6,17,21],[17,0,17,5],[20,6,20,7],[23,0,23,1],[21,6,21,21],[23,19,23,21],[23,13,23,14],[23,15,23,17],[28,36,29,42],[28,0,29,10],[23,2,23,8],[20,0,20,5],[23,9,23,10],[23,11,23,12],[24,23,25,42],[22,26,22,41],[22,6,22,21],[20,17,20,19],[11,0,11,22],[21,23,21,30],[20,9,20,10],[20,15,20,16],[20,12,20,14],[11,23,11,42],[18,0,18,5],[18,6,18,21],[19,0,19,5],[30,21,30,32],[30,33,30,35],[28,14,29,20],[28,11,29,13],[28,21,29,32],[28,33,29,35],[34,0,34,3],[35,0,35,3],[33,4,33,6],[33,0,33,3],[34,4,34,6],[35,4,35,6],[31,33,31,35],[31,14,31,20],[31,21,31,32],[31,36,31,42],[5,0,5,42],[6,0,6,42],[7,0,7,42],[8,0,10,42],[19,6,19,21],[19,23,19,25],[19,26,19,34],[16,0,16,11],[16,23,16,31],[14,23,14,39],[17,23,18,41],[26,0,26,42],[27,0,27,42],[24,0,24,5],[25,0,25,5],[25,6,25,21],[24,12,24,14],[24,6,24,7],[24,9,24,10],[33,19,33,24],[33,25,33,30],[20,23,20,25],[20,26,20,39],[32,0,32,42],[30,0,30,10],[31,0,31,10],[30,14,30,20],[30,11,30,13],[31,11,31,13],[33,31,33,36],[33,37,33,42],[34,7,34,12],[34,13,34,18],[34,19,34,24],[34,25,34,30],[34,31,34,36],[34,37,34,42],[33,7,33,12],[33,13,33,18],[39,19,40,30],[39,31,40,42],[35,7,35,12],[35,13,35,18],[35,19,35,24],[35,25,35,30],[45,0,45,42],[44,14,44,18],[44,0,44,2],[44,31,44,42],[46,0,47,42],[44,19,44,30],[41,3,41,13],[42,3,42,13],[43,3,43,13],[44,3,44,13],[42,31,42,42],[43,31,43,42],[41,0,41,2],[41,14,41,18],[42,14,42,18],[43,14,43,18],[41,19,41,30],[42,19,42,30],[43,19,43,30],[13,0,13,6],[13,7,13,14],[0,0,0,42],[41,31,41,42],[35,31,35,36],[35,37,35,42],[36,0,36,42],[38,0,38,42],[39,0,40,13],[39,14,40,18]],"flags":["formulas_cached_only"]}
["This form may be submitted to the EIA by mail, fax, e-mail, or secure file transfer.  Should you choose to submit your data via e-mail, we must advise you that e-mail is an insecure means of transmission because the data are not encrypted, and there is some possibility that your data could be compromised.  You can also send your Excel files to EIA  using a secure method of transmission: HTTPS.  This is an industry standard method to send information over the web using secure, encrypted processes.  (It is the same method that commercial companies communicate with customers when transacting business on the web.)  To use this service, we recommend the use of Microsoft Internet Explorer 5.5 or later or Netscape 4.77 or later.  Send your surveys using this secure method at:  https://idc.eia.doe.gov/upload/noticeoog.jsp"]
[{"$nulls":42},"OMB No. 1905-0165"]
[{"$nulls":42},"Expiration Date:  12/31/2009"]
[{"$nulls":42},"Version No.:  2007.01"]
[]
["FORM EIA-820"]
["ANNUAL REFINERY REPORT"]
["REPORT YEAR 2007"]
["This report is mandatory under the Federal Energy Administratino Act of 1974 (Public Law 93-275).  Failure to comply may result in criminal fines, civil penalties and other sanctions as provided by law.  Title 18 USC 1001 makes it a criminal offense for any person knowingly and willingly to make to any Agency or Department of the United States any false, fictitious, or fraudulent statements as to any matter within its jurisdiction.  See Instructions for further details on the sanctions and the provisions concerning the confidentiality of information submitted on this form."]
[]
[]
["PART 1.  RESPONDENT IDENTIFICATION ",{"$nulls":22},"PART 2.  SUBMISSION/RESUBMISSION INFORMATION"]
[]
["EIA ID NUMBER:"]
[{"$nulls":23},"If this is a resubmission, enter an \"X\" in the box:"]
["If any Respondent Identification Data has changed since the last",{"$nulls":22},"A completed form must be received by February 15, 2007 "]
["    report, enter an \"X\" in the box:"]
["Company Name:",{"$nulls":22},"Forms may be submitted using one of the following methods:"]
["Refinery Name:"]
["Contact Name:",{"$nulls":22},"Fax:",null,null,"(202) 586-1076"]
["Phone No.:",{"$nulls":7},"-",null,null,"-",null,null,null,"Ext:",{"$nulls":7},"Email:",null,null,"OOG.SURVEYS@eia.doe.gov"]
["Address 1:",{"$nulls":22},"Secure File Transfer:"]
["Address 2:",{"$nulls":25},"https://idc.eia.doe.gov/upload/noticeoog.jsp"]
["City:",{"$nulls":8},"State:",null,null,null,"Zip:",{"$nulls":4},"-"]
["Fax No.:",{"$nulls":7},"-",null,null,"-",{"$nulls":11},"Questions? Call (202) 586-6281"]
["Email address:"]
[]
["PART 3. FUEL, ELECTRICITY, AND STEAM PURCHASED & CONSUMED AT THE REFINERY DURING 2006"]
["Item",{"$nulls":10},"Code",null,null,"Quantity Used As Fuel",{"$nulls":6},"Item",{"$nulls":11},"Code",null,null,"Quantity Used As Fuel"]
[]
["Natural Gas (million cubic feet)",{"$nulls":10},105,{"$nulls":9},"Purchased Electricity (million kWh)",{"$nulls":11},114]
["Coal (thousand short tons)",{"$nulls":10},109,{"$nulls":9},"Purchased Steam (million pounds)",{"$nulls":11},113]
["PART 4.  REFINERY RECEIPTS OF CRUDE OIL BY METHOD OF TRANSPORTATION DURING 2006 (Thousand Barrels)"]
["Source",null,null,null,"Code",null,null,"Pipelines",{"$nulls":5},"Tankers",{"$nulls":5},"Barges",{"$nulls":5},"Tank Cars",{"$nulls":5},"Trucks",{"$nulls":5},"Total 1/"]
["Domestic",null,null,null,"010"]
["Foreign",null,null,null,"020"]
["1/ Total Domestic and Total Foreign Refinery Receipts (Codes 010 and 020) must equal the sum of the comparable refinery receipts on the Form EIA-810, \"Monthly Refinery Report,\" filed for January through December 2006."]
[]
["PART 5.  ATMOSPHERIC CRUDE OIL DISTILLATION CAPACITY AS OF JANUARY 1"]
["Atmospheric Crude Oil Distillation Capacity",{"$nulls":13},"Code",{"$nulls":4},"Barrels per Calendar Day 2/",{"$nulls":11},"Barrels per Stream Day"]
[]
["2007:",null,null,"Operating",{"$nulls":10},399]
[null,null,null,"Idle",{"$nulls":10},400]
[null,null,null,"Total Operable",{"$nulls":10},401]
["2008:",null,null,"Operable",{"$nulls":10},501]
["2/ Barrels per Calendar Day Operating, Idle and Total Operable Capacity (Codes 399, 400 and 401) must match the comparable capacity numbers reported on the Form EIA-810, \"Monthly Refinery Report,\" filed for January 2007."]
["Comments:  (Explain any unusual or substantially different aspects of your current year's operations that affect the data reported.)  For example, note new processing units, major modifications or retirement of processing units, sale of refinery, etc.  (To separate one comment from another, press ALT+ENTER)"]

{"sheet":"Part 6","index":1,"n_rows":42,"n_cols":34,"rows_kept":42,"cut":false,"hidden":false,"merged":[[26,0,26,12],[37,13,37,15],[35,16,35,21],[31,0,31,12],[30,0,30,12],[30,16,30,21],[33,16,33,21],[32,13,32,15],[33,13,33,15],[34,13,34,15],[22,0,22,12],[23,0,23,12],[24,0,24,12],[25,0,25,12],[27,13,27,15],[30,13,30,15],[31,13,31,15],[22,13,22,15],[27,0,27,12],[17,16,17,21],[17,22,17,27],[17,28,17,33],[19,0,19,12],[18,13,18,15],[18,16,18,21],[18,22,18,27],[18,28,18,33],[18,0,18,12],[19,28,19,33],[19,13,19,15],[20,13,20,15],[19,16,19,21],[19,22,19,27],[20,16,20,21],[20,22,20,27],[20,28,20,33],[39,28,39,33],[25,13,25,15],[26,13,26,15],[23,13,23,15],[23,16,23,21],[32,16,32,21],[32,22,32,27],[32,28,32,33],[35,13,35,15],[36,13,36,15],[39,13,39,15],[40,13,40,15],[39,16,39,21],[39,22,39,27],[40,16,40,21],[40,22,40,27],[16,0,16,12],[17,0,17,12],[15,0,15,12],[21,0,21,12],[20,0,20,12],[28,0,29,12],[39,0,39,12],[40,0,40,12],[41,0,41,12],[32,0,32,12],[33,0,33,12],[34,0,34,12],[38,0,38,12],[35,0,35,12],[36,0,36,12],[37,0,37,12],[6,0,6,33],[7,0,7,33],[8,0,8,33],[16,13,16,15],[14,28,14,33],[13,28,13,33],[15,28,15,33],[16,28,16,33],[13,0,14,12],[12,0,12,33],[13,13,14,15],[15,13,15,15],[9,0,11,5],[10,6,10,15],[41,13,41,15],[14,16,14,21],[13,16,13,21],[14,22,14,27],[13,22,13,27],[15,16,15,21],[15,22,15,27],[16,16,16,21],[16,22,16,27],[17,13,17,15],[21,16,21,21],[21,22,21,27],[21,28,21,33],[22,28,22,33],[22,16,22,21],[22,22,22,27],[23,28,23,33],[24,16,24,21],[24,22,24,27],[24,28,24,33],[23,22,23,27],[25,16,25,21],[25,22,25,27],[25,28,25,33],[26,16,26,21],[26,22,26,27],[26,28,26,33],[27,16,27,21],[27,22,27,27],[27,28,27,33],[28,16,29,21],[28,22,29,27],[28,28,29,33],[30,28,30,33],[31,16,31,21],[31,22,31,27],[31,28,31,33],[30,22,30,27],[33,28,33,33],[34,16,34,21],[34,22,34,27],[34,28,34,33],[33,22,33,27],[35,28,35,33],[36,16,36,21],[36,22,36,27],[36,28,36,33],[35,22,35,27],[37,22,37,27],[37,28,37,33],[38,16,38,21],[38,22,38,27],[38,28,38,33],[37,16,37,21],[40,28,40,33],[41,16,41,21],[41,22,41,27],[41,28,41,33]],"flags":["formulas_cached_only"]}
[{"$nulls":33},"OMB No. 1905-0165"]
[{"$nulls":33},"Expiration Date:  12/31/2009"]
[{"$nulls":33},"Version No.:  2007.01"]
[]
[]
[]
["FORM EIA-820"]
["ANNUAL REFINERY REPORT"]
["REPORT YEAR 2007"]
["EIA ID NUMBER:"]
[{"$nulls":16},"RESUBMISSION:"]
[]
["PART 6.  DOWNSTREAM CHARGE CAPACITY AS OF JANUARY 1"]
["Downstream Charge Capacity",{"$nulls":12},"Code",null,null,2007,{"$nulls":5},2007,{"$nulls":5},2008]
[{"$nulls":16},"Barrels per Calendar Day",{"$nulls":5},"Barrels per Stream Day",{"$nulls":5}," Barrels per Stream  Day"]
["Vacuum Distillation",{"$nulls":12},402]
["Thermal Cracking:"]
["   Visbreaking",{"$nulls":12},403]
["   Fluid Coking (incl. Flexicoking)",{"$nulls":12},404]
["   Delayed Coking",{"$nulls":12},405]
["   Other (incl. Gas Oil)",{"$nulls":12},406]
["Catalytic Cracking:"]
["   Fresh Feed",{"$nulls":12},407]
["   Recycled",{"$nulls":12},408]
["Catalytic Hydrocracking:"]
["    Distillate",{"$nulls":12},439]
["    Gas Oil",{"$nulls":12},440]
["    Residual",{"$nulls":12},441]
["Desulfurization (including Catalytic Hydrotreating):"]
[]
["   Naphtha/Reformer Feed",{"$nulls":12},426]
["   Gasoline",{"$nulls":12},420]
["   Kerosene and Jet",{"$nulls":12},421]
["   Diesel Fuel",{"$nulls":12},422]
["   Other Distillate",{"$nulls":12},423]
["   Residual",{"$nulls":12},424]
["   Heavy Gas Oil",{"$nulls":12},413]
["   Other",{"$nulls":12},425]
["Catalytic Reforming:"]
["   Low Pressure",{"$nulls":12},430]
["   High Pressure",{"$nulls":12},431]
["Fuels Solvent Deasphalting",{"$nulls":12},432]

{"sheet":"Part 7-8","index":2,"n_rows":53,"n_cols":34,"rows_kept":53,"cut":false,"hidden":false,"merged":[[40,25,40,33],[37,16,37,24],[37,25,37,33],[38,16,38,24],[38,25,38,33],[39,25,39,33],[39,16,39,24],[23,25,23,33],[25,16,25,24],[25,25,25,33],[27,25,27,33],[26,16,26,24],[26,25,26,33],[27,16,27,24],[16,16,16,24],[17,13,17,15],[19,25,19,33],[20,16,20,24],[20,25,20,33],[18,25,18,33],[18,13,18,15],[16,13,16,15],[19,13,19,15],[20,13,20,15],[13,13,14,15],[15,13,15,15],[14,16,14,24],[13,16,13,24],[15,16,15,24],[9,0,11,5],[6,0,6,33],[7,0,7,33],[8,0,8,33],[10,17,10,22],[9,16,11,16],[14,25,14,33],[13,25,13,33],[15,25,15,33],[16,25,16,33],[13,0,14,12],[12,0,12,33],[48,16,48,24],[48,25,48,33],[41,25,41,33],[42,25,42,33],[43,16,43,24],[43,25,43,33],[44,16,44,24],[44,25,44,33],[49,0,50,33],[52,0,53,33],[46,16,46,24],[46,25,46,33],[47,16,47,24],[47,25,47,33],[47,13,47,15],[48,13,48,15],[46,13,46,15],[45,16,45,24],[45,25,45,33],[43,13,43,15],[44,13,44,15],[45,13,45,15],[40,13,40,15],[41,13,41,15],[42,13,42,15],[41,16,41,24],[42,16,42,24],[40,16,40,24],[38,13,38,15],[29,16,29,24],[29,25,29,33],[24,0,24,33],[25,0,25,12],[25,13,25,15],[26,13,26,15],[30,25,30,33],[31,16,31,24],[31,25,31,33],[37,13,37,15],[35,13,35,15],[36,13,36,15],[28,16,28,24],[32,16,32,24],[30,16,30,24],[34,16,34,24],[33,16,33,24],[36,16,36,24],[35,16,35,24],[21,13,21,15],[23,13,23,15],[35,25,35,33],[36,25,36,33],[22,13,22,15],[23,16,23,24],[28,25,28,33],[32,25,32,33],[33,25,33,33],[34,25,34,33],[21,25,21,33],[22,16,22,24],[17,16,17,24],[17,25,17,33],[18,16,18,24],[22,25,22,33],[19,16,19,24],[21,16,21,24],[39,1,39,12],[27,13,27,15],[28,13,28,15],[29,13,29,15],[30,13,30,15],[31,13,31,15],[32,13,32,15],[33,13,33,15],[34,13,34,15],[39,13,39,15]],"flags":["formulas_cached_only"]}
[{"$nulls":33},"OMB No. 1905-0165"]
[{"$nulls":33},"Expiration Date:  12/31/2009"]
[{"$nulls":33},"Version No.:  2007.01"]
[]
[]
[]
["FORM EIA-820"]
["ANNUAL REFINERY REPORT"]
["REPORT YEAR 2007"]
["EIA ID NUMBER:"]
[{"$nulls":17},"RESUBMISSION:"]
[]
["PART  7.  PRODUCTION CAPACITY AS OF JANUARY 1 (Barrels per Stream Day, Except Where Noted)"]
["Production Capacity",{"$nulls":12},"Code",null,null,2007,{"$nulls":8},2008]
[{"$nulls":16},"Barrels per Stream Day",{"$nulls":8}," Barrels per Stream  Day"]
["Alkylates",{"$nulls":12},415]
["Aromatics",{"$nulls":12},437]
["Asphalt and Road Oil",{"$nulls":12},931]
["Isobutane (C4)",{"$nulls":12},615]
["Isopentane (C5), Isohexane (C6)",{"$nulls":12},438]
["Lubricants",{"$nulls":12},854]
["Petroleum Coke - Marketable",{"$nulls":12},"021"]
["Hydrogen(million cubic ft. per day)",{"$nulls":12},"091"]
["Sulfur (short tons)",{"$nulls":12},435]
["PART 8.  STORAGE CAPACITY AS OF JANUARY 1, 2007 (Thousand Barrels)"]
["Storage Capacity",{"$nulls":12},"Code",null,null,"Working",{"$nulls":8},"Shell"]
["Crude Oil",{"$nulls":12},"050"]
["Motor Gasoline:"]
[null,"Reformulated",{"$nulls":11},150]
[null,"Conventional",{"$nulls":11},152]
[null,"Gasoline Blending Components",{"$nulls":11},136]
["Oxygenates:"]
[null,"Fuel Ethanol (FE)",{"$nulls":11},141]
[null,"Ethyl Tertiary Butyl Ether (ETBE)",{"$nulls":11},142]
[null,"Methyl Tertiary Butyl Ether (MTBE)",{"$nulls":11},144]
[null," Other Oxygenates*",{"$nulls":11},445]
["Kerosene",{"$nulls":12},311]
["Distillate Fuel Oil:"]
[null,"15 ppm sulfur and under",{"$nulls":11},465]
[null,"Greater than 15 to 500 ppm sulfur",{"$nulls":11},466]
[null,"Greater than 500 ppm sulfur",{"$nulls":11},467]
["Residual Fuel Oil",{"$nulls":12},511]
["Kerosene-Type Jet Fuel",{"$nulls":12},213]
["Propane/Propylene",{"$nulls":12},231]
["Normal Butane/Butylene",{"$nulls":12},232]
["Lubricants",{"$nulls":12},854]
["Asphalt and Road Oil",{"$nulls":12},931]
["Other**",{"$nulls":12},333]
["Total Storage Capacity",{"$nulls":12},999]
["* Includes other aliphatic alcohols and ethers intended for motor gasoline blending (e.g., isopropyl ether (IPE), n-propanol,  TAME, and TBA)."]
[]
[]
["** Includes ethane/ethylene, isobutane/isobutylene, pentanes plus, other hydrocarbons, hydrogen, unfinished oils, finished aviation gasoline, special naphthas, wax, petroleum coke, still gas, petrochemical feedstocks and miscellaneous products."]